

BUILDER’S ONE YEAR LIMITED WARRANTY
1. Term and Standards The term of this limited warranty is exactly one year, beginning on the date of this Agreement. The Builder warrants that the Building will be free from defects in workmanship and materials consistent with applicable building codes and the NAHB Residential Construction Performance Guidelines in effect at the time of construction. These specific NAHB Guidelines shall serve as the sole benchmark for determining the existence of a defect and shall supersede any other "generally accepted industry standards" or subjective expectations. This warranty is strictly limited to the correction of structural errors and material failures and is not to be construed as a maintenance warranty.
2. Coverage and Payment Conditions Builder shall repair or replace, at Builder’s sole option, covered defects that fail to meet NAHB standards. For Sealed Concrete Floors, only cracks exceeding 3/16 inch in width or vertical displacement are covered. For Foundations, only cracks exceeding 1/4 inch in width or those allowing water to enter a conditioned crawlspace or basement are covered. Repairs to concrete will be visible and are not guaranteed to match original color or texture. This warranty is void and unenforceable unless payment in full is made to the Builder on or before the date of this Agreement. No funds shall be withheld by the Owner for items covered by this warranty.

3. Exclusions The following items are expressly excluded from coverage:
· Owner Maintenance: Damage due to abuse, neglect, or failure to provide proper maintenance, including the failure to disconnect hoses in freezing temperatures.
· Grading and Drainage: Settling of the ground around the foundation and utility locations is a natural occurrence and is excluded. Per NAHB standards, proper drainage is defined as water not standing in yard areas (outside of designated swales) for more than 48 hours after a rain event. Any adjustments to grading by the Owner void this portion of the warranty.
· Landscaping: All sod, seeding, shrubs, trees, plantings, and sprinkler systems.
· Surface Damage: Damage to walls, cabinets, counters, and flooring is excluded unless documented in writing during the walkthrough inspection at the time of closing.
· Consequential Damages: Builder is not responsible for cost of shelter, food, moving, storage, or loss of market value associated with a defect or repair.

4. Consolidated 11th-Month Repair Visit To allow for structural stabilization through seasonal changes, the Builder will perform the following cosmetic repairs one time only during the 11th month following the date of this Agreement:
· Drywall: Repair of nail pops or ridges exceeding 1/8 inch in depth or projection.
· Caulking: Re-caulking of interior or exterior trim joints that exceed 1/4 inch in separation.
· Touch-up Paint: Painting is limited to repaired areas only; an exact color match is not guaranteed due to normal fading and lapse of time.

5. Mechanical and Plumbing
· Pipe Noise: Ticking or knocking sounds due to thermal expansion are normal characteristics and not defects. Only specific "water hammer" hydraulic shock is a covered defect.
· Sump Pumps: Maintenance and continuous power supply (including backup batteries) are the sole responsibility of the Owner.
· Appliances: Warranted solely by the manufacturer; Owner must contact the manufacturer's service department directly.
6. Administrative Provisions
· Notice of Claim: Owner must provide prompt written notice of any defect and proof of delivery prior to the expiration of the one-year term.
· Access: Owner shall provide Builder and its agents reasonable access during normal working hours and clear all furniture or obstacles from the repair area.
· Transferability: This warranty is not assignable or transferable to any subsequent owner.




